***Blinking LED Using ESP32 On Wokwi Simulation***

#include <Arduino.h>

const int ledPin = 2; // LED connected to GPIO2

void setup() {

  pinMode(ledPin, OUTPUT); // Set the LED pin as an output

}

void loop() {

  digitalWrite(ledPin, HIGH); // Turn the LED on

  delay(1000);              // Wait for 1 second

  digitalWrite(ledPin, LOW);  // Turn the LED off

  delay(1000);              // Wait for 1 second

}



